# Special Inspections for Wind Resistance

See the Schedule of Special Inspections for inspection and testing requirements

**Allowable Stress Design Wind Speed, Vasd: m.p.h.**

**Wind Exposure Category:**

**Special Inspection for Wind Resistance Required (Yes/No):**

(Required in wind exposure Category B, where the allowable stress design wind speed, Vasd, is 120 miles per hour or greater. Required in wind exposure Category C or D, where the allowable stress design wind speed, Vasd, is 110 miles per hour or greater).)

Description of structural wood and cold-formed steel light frame construction main windforce-resisting system subject to special inspections for wind resistance:

(Required for systems noted in IBC Section 1705.11.1 and 1705.11.2).

Description of windforce-resisting components subject to special inspections for wind resistance:

(Required for systems and components noted in IBC Section 1705.11.3)

**Statement of Responsibility:**

Each contractor responsible for the construction or fabrication of a system or component described above must submit a Statement of Responsibility.